|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Fill the Information Below** | | | | | | | | |
| Company: **Rezayat Company Limited** | | | | | Date: 5/24/2021 | | | |
| Location: Area 2 | | | | | Time: 05.30 PM | | | |
| Project/ Site Name: Catering Auditorium & Recreation Facilities : **097-C76R** | | | | | Worst Potential Severity: 4 Actual Severity: 2 | | | |
| **Person(s) Involved:** |  | **Employee** | **✓** | **Contractor** |  | **Others** | |  |
| 1. Jaginder | | | 3. | | | | | |
| 2.Barath | | | Other(s). | | | | | |
| **Type of Incident:** | | | | | | | | |
| Near Miss | | | | | | | | |
| **Injury Location by Body Parts (Select one or more if necessary):** | | | | | | | | |
| Head |  | Chest |  | Hand |  | Eyes |  | |
| Face |  | Leg |  | Arm |  | Hip |  | |
| Neck |  | Abdomen |  | Wrist |  | Ankle/Foot |  | |
| Back |  | Stomach |  | Elbow |  | Knee |  | |
| Nose/ Ears |  | Shoulder |  | Fingers/ Thumb |  | Toes |  | |
| **Type of Injury Sustained (Select one or more if necessary):** | | | | | | | | |
| Fracture |  | Cut/ Laceration |  | Scalping |  | Bruising |  | |
| Loss of Sight |  | Loss of Consciousness |  | Heat |  | Amputation |  | |
| Dislocation |  | Crush Injury |  | Cold |  | Other(s) |  | |
| Abrasion |  | Suffocation |  | Burn |  |  |  | |
| **Immediate Cause(s) (Select one or more if necessary):** | | | | | | | | |
| Safety Rule Violated |  | Lack of Resources |  | Drugs/ Alcohol Related |  | Inadequate Visibility |  | |
| Lack of Task Skill |  | Method Deviation |  | Poor Housekeeping |  | Employee Morale |  | |
| Lack of Supervision | **✓** | Poor Weather Conditions |  | Inadequate Lighting |  | Employee Attitude |  | |
| Improper Lifting (MH) |  | Lack of Task Knowledge |  | Poor Team Work |  | Behavior Problem |  | |
| Not Paying Attention | **✓** | Lack of Communication |  | No Risk Assessment |  | Poor Ground Conditions |  | |
| Human Error |  | Incorrect Tools/Equip |  | Defective Equipment |  | Improper Lifting (crane) |  | |
| Inadequate PPE |  | Defective Tools |  | Unprotected excavation |  | Unprotected Edge |  | |
| Animals |  | Violence |  | Horseplay |  | Improper/ Poor Slinging |  | |
| Heat Stress |  | STF Above Ground |  | STF on the Same Level |  | Manual Handling |  | |
| Misuse of Hand Tools |  | Grinding/ Welding |  | Knives/ Sharps |  | Hit by Vehicle |  | |
| Hit by Static Machinery |  | Heavy Equipment |  | Splashes from C.P.O.L. |  | Other(s) : |  | |
| Stress |  | Fatigue |  | Vandalism |  |  |  | |
| **Equipment(s) Involved:** | | | | | | | | |
| Light Vehicle: |  | Heavy Vehicle: |  | Plant Equipment: |  | Static Plant Equipment: |  | |
| Building: |  | Structure: |  | Scaffold: |  | Excavation: |  | |
| Other(s): |  |  |  |  |  |  |  | |
| **Description of the Event:** | | | | | | | | |
| During the water proofing work (using LPG cylinder and burner) in ground floor (near part 7 toilet area) filler board that was filled between wall joints, caught fire (Smoldering Fire).  Smokes were observed 1 hour after the sub-con team left the site. Fire was immediately extinguished. | | | | | | | | |
| **Immediate Action(s) Taken to Prevent Reoccurance (If Any):** | | | | | | | | |
| Fire was extinguished by pouring water on it.  Warning letter was given to concerned sub-con supervisor.  Hot work checklist must be filled before start of work.  Filler board should be made wet before start of work.  Ensure the fire extinguisher availability.  Fire watcher should check the site for one hour after finishing the hot work and ensure no signs of fire before leaving.  Strict supervision must be ensured by the sub-con team. | | | | | | | | |
| **Person Created the Report:** | | | | | | | | |
| Name: Arun K Thampy | | Position: Safety Officer | | Signature: Waqas Gillani | | Date: 5/25/2021 | | |
|  | |  | |  | |  | | |

